**Instructions To Charge the Lowrance GPS HDS5 Battery**

1. Plug in the battery charger and make sure the switch is set to 12V. The clips with black and red heads on the charger are those that will be attached to the battery (see below).
2. The Lowrance GPS Unit battery is the red box on the device. You will see two cords, one grey and one black, attached to this battery. They are attached to square metals brackets. The two clips from the battery charger are attached to these metal square brackets for charging.
3. Pull back the plastic that covers the GPS battery far enough so that the charger clips can be attached to the metal brackets; do not remove the plastic cover.
4. Attach the red clip from the charger to the metal bracket with a red base on the GPS battery. Attach the black clip from the charger to the bracket with a black base on the GPS battery.
5. Charge the battery for no more than one (1) hour. Charging for > 1 hour could overheat the GPS battery, causing an explosion.
6. When charging is complete, remove the charger clips from the metal brackets, and unplug the charger.
7. Replace the plastic cover over the battery, tucking in the flap so that it is secure.